ANNEX B:  TECHNICAL SPECIFICATIONS/OFFER FORM FOR MULTI-PURPOSE SOAP BARS



	
	Specifications
	Response
	Remarks 

	Soap Bar Type – Category (please indicate compliance with minimum and maximum tolerances per each content specification)

	1
	Chemical composition
Fatty Acid (TFM): Min. 70%
Moisture: Max. 20%
NaOH content:	Max. 0.15%
NaCl content:  Max. 0.45%  
Unsaponified/nonsaponifiable matter: Max. 2.50%
Mercury:  No Mercury Content
	
	

	Packaging (please describe in detail the nature and quality of compliance of your company’s proposed packaging) 

	1
	Mandatory: Unwrapped soap bars of 250 grams each, packed inside new/unused, strong 3 ply corrugated cartons that meet the requirement of securely holding and protecting chemical content (soap bars), suitable for multi-modal transport, suitable to withstand rough handling by long distance road transport, suitable for stacked storage of several meters high.  
	
	

	2
	Optimal: Each carton shrink wrapped in plastic binders on both sides (widthwise and lengthwise). 
	
	

	3
	Mandatory: Each box must bear UNHCR shipping marks (production batch, PO number, Supplier name) as indicated printed, spray-painted, or stickered.
	
	

	4
	Mandatory: Maximum content per carton, 20 kilogram net weight soap bars. 
	
	

	5
	Optional: Palletization, as and when requested by UNHCR, at no additional cost.
	
	

	Minimum packing unit quality control levels (please indicate which shall be applied by your company) 

	1
	Optional: Guaranteed 100% (semi-automated) quality control of each individual minimum packing unit (appearance, sealing and weight).
	
	

	2
	Optional: Weighing of complete order, before palletization.     
	
	

	3
	Mandatory: Representative sampling/random weighing of minimum units before palletization. 
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